
	
	                                                               


	
Tender text 
Motion/presence detector theMura S180 Slave UP WH
Order No. white: 		2060660

Features: 
· Passive infrared motion/presence detector for wall mounting in flush-mounted box
· Cover in Theben design
· Slave device for the extension of the detection area of theMura detectors
· Rectangular detection area 170°, max. 14 m x 17 m
· Area restriction in scope of delivery
· Integrated button (can be deactivated)
· Fully or semi-automatic operation, switchable (can be set at master)
· Staircase light function (can be set at master)
· Extended function (can be set at master)
· Ready for immediate use due to factory presetting 
· Test mode for checking the detection area

Technical data:
Operating voltage: 		230 V AC
Frequency: 			50 – 60 Hz
Power consumption: 		approx. 0.4 W
Radial detection area: 		12 x 10 m
Tangential detection area: 	14 x 17 m
Installation height Mh: 		0.8 – 1.2 m
Protection rating: 		IP20
Operating temperature: 		-15 °C to +45 °C
Dimensions: 			85 x 85 mm, installation depth 37 mm
Installation: 			wall mounting in flush-mounted box size 1
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