
	
	                                                               


	
Tender text 
Motion detector theMura S180-100 UP WH
Order No. white: 		2060650

Features: 
· Passive infra-red motion detector for wall mounting in flush-mounted box
· Cover in Theben design
· Automatic presence and brightness-dependent control for lighting 
· Rectangular detection area 170°, max. 14 m x 17 m
· Area restriction in scope of delivery
· Mixed light measurement suitable for fluorescent lamps (FL/PL/ESL), halogen/incandescent lamps and LEDs
· Integrated button (can be deactivated)
· Fully or semi-automatic operation, switchable
· Staircase light function
· Extended function
· Adjustable brightness switching value, teach-in function
· Pulse function for staircase light timer switch
· Ready for immediate use due to factory presetting 
· Test mode for checking the detection area
· Extension of detection area via master/slave switching

Technical data:
Operating voltage: 		      230 V AC
Frequency: 			      50 – 60 Hz
Power consumption: 		      approx. 0.4 W
Radial detection area: 		      12 x 10 m
Tangential detection area: 	      14 x 17 m
Installation height Mh: 		      0.8 – 1.2 m
Channel A Light: 		      relay, 1 NO contact 230 V / 10 A, 2300 W or 1150 VA (cos ϕ = 0.5)
Switching capacity LED < 2 W:     typ. 40 W
Switching capacity LED > 2 W:     typ. 450 W
Brightness switching value: 	      5 – 1000 lux
Lighting time delay: 		      10 s – 30 min, pulse
Protection rating: 		      IP20
Operating temperature: 		      -15 °C to +45 °C
Dimensions: 			      85 x 85 mm, installation depth 37 mm
Installation: 			      wall mounting in flush-mounted box size 1








Optional accessories:

Extension of detection area via slave device:
Order No. white: 		2060660 (theMura S180 Slave UP WH)
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