Hygrostat for wall installation (SOTHIS 715)
	
Hygrostat for wall installation; housing 74 x 74mm; depth 28mm; setting range 35-100% fF;  wall mounting 74 x 74 x 28 mm; 1 two way switch; humidifier 2
A/250V~; dehumidifier 5 A/250V~

Deliver, assemble, connect up and set up
...

Make: Theben

Type: SOTHIS 715
Order No.: 7150002

Unit: ST

