Rail mounted-elapsed-time counter, 2 TLE (BZ 145)

Rail mounted elapsed-time counter; width 35 mm; terminal screws; counter range up to 99,999.9 hours; operating voltage 230 V~/ 50 Hz

Deliver, assemble, connect up and set up
...

Make: Theben

Type: BZ 145
Order No.: 1450000

Unit: ST

