Rail mounted staircase light timer with synchronous motor (ELPA 8)

Rail mounted staircase timer; width 17.5 mm; time range 1 - 7 minutes; can be retriggered; max. 50 mA glow lamp load; 3 and 4 wire connection; continuous light function; 1 NO contact 16 (6)A/230V~

Deliver, assemble, connect up and set up
...

Make: Theben

Type: ELPA 8
Order No.: 0080002

Unit: ST

