EIB/KNX secondary clock, single-sided wall clock (OSIRIA 251 BQ-EIB/KNX)
	
EIB/KNX secondary clock for schools and sports halls; limited protected against thrown balls; single-sided internal wall clock; square clock face 40 x 40cm; white metal face with black Arabic numerals; printing in accordance with DIN 41 09; laminated safety glass; very stable metallic housing; dimensions 40 x 40 cm; height 10 cm

Deliver, assemble, connect up and set up
...

Make: Theben

Type: OSIRIA 251 BQ-EIB/KNX
Order No.: 5009252

Unit: ST

