Rail mounted 24 hour timer, pins, 1 TLE (SYN 160 a)

Rail mounted timer without power reserve; width 17.5mm; 24 hour segment program; shortest switching time 15 minutes.; Permanent ON/OFF switching; 1 NO contact 16A/250V~; sealable transparent cover.

Deliver, assemble, connect up and set up
...

Make: Theben

Type: SYN 160 a
Order No.: 1600001

Unit: ST

